;; netrtwlans.inf 
;;
;; Realtek Wireless 802.11b/g/n SDIO Network Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlans.cat		;; for WHQL certified
DriverVer = 01/14/2016,3008.25.1216.2015

[Manufacturer]
%Realtek% = Realtek,NTx86.10.0


[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTx86.10.0]

;; For 8723 RTK common		================================================================

;; For 8723 RTK common		================================================================
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_8753
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_B723
;; Acer
%RTL8723bs.DeviceDesc% = ACER8723bs.ndi, SD\VID_024C&PID_0623
;; HP
%RTL8723bs.DeviceDesc% = HP8723bs.ndi, SD\VID_024C&PID_0523
;; ECS
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_0524
;; bestbuy
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_0240
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_0241
;; For Braswell platform
%RTL8723bs.DeviceDesc% = RTL8723bs.ndi, SD\VID_024C&PID_0626
;; Reserved
%RTL8723bs.DeviceDesc% = RSVD8723bs.ndi, SD\VID_024C&PID_0624

;; For 8188E RTK common		================================================================
%RTL8188es.DeviceDesc% = RTL8188es.ndi, SD\VID_024C&PID_8188
%RTL8188es.DeviceDesc% = RTL8188es.ndi, SD\VID_024C&PID_8179 

;; For 8812A RTK common		================================================================

;; For 8814A RTK common		================================================================
%RTL8814as.DeviceDesc% = RTL8814as.ndi, SD\VID_024C&PID_8813

;; For 8821A RTK common		================================================================
%RTL8821as.DeviceDesc% = RTL8821as.ndi, SD\VID_024C&PID_8821

;; For 8192ES RTK common		================================================================
%RTL8192es.DeviceDesc% = RTL8192es.ndi, SD\VID_024C&PID_818B


;; For 8703 RTK common		================================================================
%RTL8703bs.DeviceDesc% = RTL8703bs.ndi, SD\VID_024C&PID_B703

;; For 8188 RTK common		================================================================
%RTL8188fs.DeviceDesc% = RTL8188fs.ndi, SD\VID_024C&PID_F179

;; For 8822B RTK common		================================================================
%RTL8822bs.DeviceDesc% = RTL8822bs.ndi, SD\VID_024C&PID_B822

;; For 8821C RTK common		================================================================
%RTL8821cs.DeviceDesc% = RTL8821cs.ndi, SD\VID_024C&PID_B821

;; For 8723D RTK common		================================================================
%RTL8723ds.DeviceDesc% = RTL8723ds.ndi, SD\VID_024C&PID_D723

;;----------------------------------------------------------------------------
;; Realtek 8723as default installation
;;----------------------------------------------------------------------------

             



[RTL8723as.ndi.NT]
AddReg				= NDIS_64.reg, RTL8723as.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723as.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723as.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8723bs default installation
;;----------------------------------------------------------------------------

             



[RTL8723bs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8723bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, AutoChnlSelon.reg, CIHVS.reg, MCC.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
;;----------------------------------------------------------------------------
;; Acer 8723bs installation
;;----------------------------------------------------------------------------

             



[ACER8723bs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8723bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, AutoChnlSelon.reg, CIHVS.reg, RSSI2GridMode_2.reg, MCC.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[ACER8723bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[ACER8723bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
;;----------------------------------------------------------------------------
;; HP 8723bs installation
;;----------------------------------------------------------------------------

             



[HP8723bs.ndi.NT]
AddReg				= NDIS_64.reg, HP8723bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, AutoChnlSelon.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[HP8723bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[HP8723bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; RSVD 8723bs installation
;;----------------------------------------------------------------------------

             



[RSVD8723bs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8723bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, WowlanDisable.reg, 32kEnable.reg, AutoChnlSelon.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RSVD8723bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RSVD8723bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8188eu default installation
;;----------------------------------------------------------------------------





[RTL8188es.ndi.NT]
AddReg				= NDIS_64.reg, RTLWLAN.reg, 11nWirelessMode.reg, Ndis6Set.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188es.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188es.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8821as default installation
;;----------------------------------------------------------------------------





[RTL8821as.ndi.NT]
AddReg				= NDIS_64.reg, RTL8821as.common.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6Set.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821as.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821as.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8814as default installation
;;----------------------------------------------------------------------------





[RTL8814as.ndi.NT]
AddReg				= NDIS_64.reg, RTL8814as.common.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6Set.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8814as.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8814as.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8192es default installation
;;----------------------------------------------------------------------------





[RTL8192es.ndi.NT]
AddReg				= NDIS_64.reg, RTL8192es.common.reg, RTLWLAN.reg, 11nWirelessMode.reg, Ndis6Set.reg, CIHVS.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192es.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192es.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8703bs default installation
;;----------------------------------------------------------------------------

             



[RTL8703bs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8703bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, AutoChnlSelon.reg, CIHVS.reg, KFREE_COMMON.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8703bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8703bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8188fs default installation
;;----------------------------------------------------------------------------

             



[RTL8188fs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8703bs.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, CIHVS.reg, PnpPreTransOn.reg, AutoChnlSelon.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188fs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188fs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8822bs default installation
;;----------------------------------------------------------------------------





[RTL8822bs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8822bs.common.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6Set.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8822bs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8822bs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 88221cs default installation
;;----------------------------------------------------------------------------





[RTL8821cs.ndi.NT]
AddReg				= NDIS_64.reg, RTL8821cs.common.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6Set.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821cs.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821cs.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;----------------------------------------------------------------------------
;; Realtek 8723ds default installation
;;----------------------------------------------------------------------------





[RTL8723ds.ndi.NT]
AddReg				= NDIS_64.reg, RTL8723ds.common.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, ConnectedStandbyEnable.reg, 32kEnable.reg, CIHVS.reg, PnpPreTransOn.reg, AutoChnlSelon.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanS.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723ds.ndi.NT.Services]
AddService			= RtlWlans, 2, RtlWlans.Service, RtlWlans.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723ds.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; OS relative registry.
;;----------------------------------------------------------------------------
[NDIS_64.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan,ethernet,vwifi"
HKR, Ndi,				Service,    0, "RtlWlans"
;;
;; OS relative service.
;;
[RtlWlans.Service]
DisplayName    	= %RtlWlans.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\rtwlans.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlans.EventLog]
AddReg 			= RtlWlans.AddEventLog.reg

[RtlWlans.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;*******************************************************************************
; WAPI section
;*******************************************************************************
[wapi.reg]
HKR,defaults,WapiSupport,0,"1"
HKR,,WapiSupport,0,"1"

;*******************************************************************************
; RTL8723as common paramters
;*******************************************************************************
[RTL8723as.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"


;*******************************************************************************
; RTL8723bs common paramters
;*******************************************************************************
[RTL8723bs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,RomDLFwEnable,0,"1"
HKR,,RomDLFwEnable,0,"1"

HKR,defaults,bFwCtrlPwrOff,0,"1"
HKR,,bFwCtrlPwrOff,0,"1"

;;HKR,defaults,EnableAdaptivity,0,"0"
;;HKR,,EnableAdaptivity,0,"0"

HKR,defaults,EnableCarrierSense,0,"0"
HKR,,EnableCarrierSense,0,"0"

;; $$ End of RTL8723bs.common.reg

[HP8723bs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,RomDLFwEnable,0,"1"
HKR,,RomDLFwEnable,0,"1"

HKR,defaults,bFwCtrlPwrOff,0,"1"
HKR,,bFwCtrlPwrOff,0,"1"

; Enable Adaptivity
;;HKR,defaults,EnableAdaptivity,0,"1"
;;HKR,,EnableAdaptivity,0,"1"

HKR,defaults,EnableCarrierSense,0,"0"
HKR,,EnableCarrierSense,0,"0"

; Enable Customeized PowerLimit Table
HKR,,EnableTxPowerLimit,0,"1"
HKR,,DecryptCustomFile,,"1"
HKR,,PwrLimitFile,0,"TXPWR_LMT_IEC0921_Enc.txt"

; Regulation WorldWide
HKR,defaults,PwrTblSel,0,"4"
HKR,,PwrTblSel,0,"4"

;; $$ End of HP8723bs.common.reg

;*******************************************************************************
; RTL8703bs common paramters
;*******************************************************************************
[RTL8703bs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,RomDLFwEnable,0,"1"
HKR,,RomDLFwEnable,0,"1"

HKR,defaults,bFwCtrlPwrOff,0,"1"
HKR,,bFwCtrlPwrOff,0,"1"


;*******************************************************************************
; RTL8188Fs common paramters
;*******************************************************************************
[RTL8188fs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,RomDLFwEnable,0,"0"
HKR,,RomDLFwEnable,0,"0"

HKR,defaults,bFwCtrlPwrOff,0,"1"
HKR,,bFwCtrlPwrOff,0,"1"


;*******************************************************************************
; RTL8821as common paramters
;*******************************************************************************
[RTL8821as.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

HKR,,StbcCap,0,"17"
HKR,,LdpcCap,0,"34"
HKR,,BeamformCap,0,"34"


;*******************************************************************************
; RTL8814as common paramters
;*******************************************************************************
[RTL8814as.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

;; Add for 8814AS, based on 8821AS's modification
HKR,,StbcCap,0,"17"
HKR,,LdpcCap,0,"34"
HKR,,BeamformCap,0,"34"


;*******************************************************************************
; RTL8192es common paramters
;*******************************************************************************
[RTL8192es.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

;*******************************************************************************
; RTL8822bs common paramters
;*******************************************************************************
[RTL8822bs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

HKR,,BeamformCap,0,"34"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,TxPktBufMode,0,"2"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"


;*******************************************************************************
; RTL8821cs common paramters
;*******************************************************************************
[RTL8821cs.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

HKR,,StbcCap,0,"17"
HKR,,LdpcCap,0,"34"
HKR,,BeamformCap,0,"34"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"



;*******************************************************************************
; RTL8723ds common paramters
;*******************************************************************************
[RTL8723ds.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"

HKR,defaults,bEarlymodeEnable,0,"0"
HKR,,bEarlymodeEnable,0,"0"

HKR,defaults,LdpcCap,0,"0"

HKR,defaults,StbcCap,0,"16" 

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]

; Enable Adaptivity
HKR,,EnableAdaptivity,0,"1"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

;; Antenna Diversity Type
HKR,defaults,AntennaDivType,0,"0"
HKR,,AntennaDivType,0,"0"

HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

; For B/G mode and B/G/N mode switch, we will use different wireless mode registry in later section
HKR,Ndi\params\WirelessMode, 			ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 			type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 			default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 		"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 		"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 		"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"


;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"3"
HKR,,LPSIntvl,0,"3"

HKR,,WEPinNmode,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

HKR,defaults,NblRacingWA,0,"1"
HKR,,NblRacingWA,0,"1"

;; Rx reorder pending time
HKR,,RxReorder_PendTime,0,"100"

;Antenna Diversity
HKR,Ndi\params\AntDiv,			ParamDesc, 		0, "Antenna Diversity"
HKR,Ndi\params\AntDiv, 			default, 		0, "0"
HKR,Ndi\params\AntDiv, 			type, 		    0, "enum"
HKR,Ndi\params\AntDiv\enum,  	"0",        	0, %DISABLED_STR%
HKR,Ndi\params\AntDiv\enum,   	"1",        	0, %ENABLED_STR%

HKLM, SYSTEM\CurrentControlSet\Services\RtlWlans\Parameters, "BtAntennaInHw", 0x00010001,2

[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"


[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"


;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting, 			ParamDesc, 	0, "Bandwidth"
HKR,Ndi\params\BWSetting, 			type, 		0, "enum"
HKR,Ndi\params\BWSetting, 			default, 	0, "1"
HKR,Ndi\params\BWSetting\enum, 		"0", 		0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum, 		"1", 		0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"36"

;; RF Type
HKR,,RFType,0,"15"


HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

;;----------------------------------------------------------------------------
;; LPS 32k Control Parameters
;;----------------------------------------------------------------------------
[32kEnable.reg]
HKR,,bLowPowerEnable,0,"1"
[32kDisable.reg]
HKR,,bLowPowerEnable,0,"0"

;-------------------------------------------------------------------------------
;	PnP pre-transition handling
;-------------------------------------------------------------------------------
[PnpPreTransOn.reg]
HKR,,PreTransPnP,0,"1"
[PnpPreTransOff.reg]
HKR,,PreTransPnP,0,"0"

;;----------------------------------------------------------------------------
;; WOWLAN Control Parameters
;;----------------------------------------------------------------------------
[WowlanAllEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLED_STR%
HKR,,*WakeOnMagicPacket,0,"1"

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLED_STR%
HKR,,*WakeOnPattern,0,"1"

[WowlanDisable.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"0"
HKR,,GTKOffloadEnable,0,"0"

[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLED_STR%
HKR,,*WakeOnMagicPacket,0,"1"

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLED_STR%
HKR,,*WakeOnPattern,0,"1"

[WowlanEnableNoPatternMatch.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLED_STR%
HKR,,*WakeOnMagicPacket,0,"1"

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLED_STR%
HKR,,*WakeOnPattern,0,"0"

[WowlanEnableNoLPSNoPatternMatch.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLED_STR%
HKR,,*WakeOnMagicPacket,0,"1"

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLED_STR%
HKR,,*WakeOnPattern,0,"0"

[ConnectedStandbyEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,D2ListenIntvl,0,"4"
HKR,,NSOffloadEnable,0,"1"
HKR,,NLOEnable,0,"1"

; AOAC reconnect
HKR,,PnpKeepLink,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "0"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLED_STR%
HKR,,*WakeOnMagicPacket,0,"0"

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLED_STR%
HKR,,*WakeOnPattern,0,"1"

;; Packet coalescing should be enabled in WHCK test
HKR,defaults,*PacketCoalescing,0,"0"
HKR,,*PacketCoalescing,0,"0"

;-------------------------------------------------------------------------------
;	Auto Channel Selection
;-------------------------------------------------------------------------------
[AutoChnlSelon.reg]
HKR,,AutoChnlSel,0,"1"
[AutoChnlSeloff.reg]
HKR,,AutoChnlSel,0,"0"

;;----------------------------------------------------------------------------
;; RSSI to Grid Mode Parameters
;;----------------------------------------------------------------------------
[RSSI2GridRealMode.reg]
HKR,,RSSI2GridMode,0,"1"
[RSSI2GridMode_2.reg]
HKR,,RSSI2GridMode,0,"2"
[RSSI2GridMode_4.reg]
HKR,,RSSI2GridMode,0,"4"

;;----------------------------------------------------------------------------
;; KFREE parameters
;;----------------------------------------------------------------------------
[KFREE_COMMON.reg]
HKR,,RfKFreeEnable,0,"0"

;*******************************************************************************
; Customer reg section
;*******************************************************************************
[ScanType.reg]
HKR,defaults,PassiveScan, 0, "0"
HKR,,PassiveScan, 0, "0"

;*******************************************************************************
; Multi-Channel Concurrent section
;*******************************************************************************
[MCC.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, %MCC_STR%
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, %DISABLED_STR%
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"4", 		0, %ENABLED_STR%
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanS.CopyFiles]
rtwlans.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanS.CopyFiles	= 12
CIHVS.CopyFiles					= 11
RtlUI2.CopyFiles				= 10

;;****************************************************************************
;; Source Files
;;****************************************************************************
[CIHVS.CopyFiles]
Rtlihvs.dll,,,2

[RegisterUIExt]
11,,RtlExtUI.dll,1

[RtlUI2.CopyFiles]
RtlUI2.exe,,,2

[SourceDisksFiles]
rtwlans.sys = 1
Rtlihvs.dll = 1

[SourceDisksNames]
1=%DISKNAME%,,,


;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR				            = "SSID"
CHANNEL_STR				            = "Channel"
NETWORK_TYPE_STR			        = "Network Type"
LED_CONTROL_STR				        = "LED Control" 
POWER_SAVE_STR				        = "Power Save Mode"
WIFI_IBSS_STR				        = "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			        = "Rate Adaptive"
QOS_STR					            = "QoS"
WiFiConfg_STR	  			        = "WiFiConfg"
WMM_APSD				            = "WMM APSD"
CCX_RM_STR				            = "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			        = "Forced Priority"
HW_PARA_STR				            = "Init from HwParaFile"
THREE_WIRE_MODE_STR		            = "Three Wire Programming Mode"
BOARD_TYPE_STR			            = "Board Type"
PROTECTION_MODE_STR		            = "Protection Mode"
TPC_STR					            = "Transmit Power Control"
TPC_POLARITY_STR		            = "TPC Polarity Select"
HIGH_POWER_STR			            = "High Power Mechanism"
INIT_GAIN_STR			            = "Initial Gain State"
CW_MAX_MIN_STR			            = "Contention Window"
PSP_XLINK_STR			            = "PSP XLink Mode"
DISABLE_STR				            = "Disable"
ENABLE_STR				            = "Enable"
DISABLED_STR				            = "Disabled"
ENABLED_STR				            = "Enabled"
AUTO_STR							= "Auto"
AD_HOC_STR				            = "Ad Hoc"
INFRASTRUCTURE_STR		            = "Infrastructure"
AUTO_SELECT				            = "Auto select"
WL_MODE_STR				            = "Wireless Mode"
RX_REORDER_STR			            = "Rx Reorder"
CAM_STR					            = "CAM"
MAX_PSP_STR				            = "MAX_PSP"
Fast_PSP_STR				        = "Fast_PSP"
NO_AC_STR					        = "No AC (Disable)"
ALL_AC_STR				            = "ALL AC"
IEEE_802_11A_STR 					= "IEEE 802.11a"
IEEE_802_11B_STR 			        = "IEEE 802.11b"
IEEE_802_11BG_STR 			        = "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			        = "IEEE 802.11b/g/n"
IEEE_802_11AN_STR					= "IEEE 802.11a/n"	
IEEE_802_11ANAC_STR					= "IEEE 802.11a/n/ac"
IEEE_802_11AC_STR					= "IEEE 802.11 ac"
WakeOnMagicPacket					= "Wake on Magic Packet"
WakeOnPattern						= "Wake on Pattern Match"                                                 
MCC_STR								= "Multi-Channel Concurrent"

;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					            = "Realtek Semiconductor Corp."


;*******************************************************************************
;	Source disk name
;*******************************************************************************
DISKNAME							= "Realtek Wireless LAN 802.11n SDIO Network Adapter Driver Disk"
RtlWlans.DeviceDesc 				= "Realtek Wireless LAN 802.11n SDIO Network Adapter"
RtlWlans.DeviceDesc.DispName		= "Realtek Wireless LAN 802.11n SDIO Network Adapter"

;*******************************************************************************
; RTL8723as Device description
;*******************************************************************************
RTL8723as.DeviceDesc 				= "Realtek RTL8723AS Wireless LAN 802.11n SDIO Network Adapter"
RTL8723as.DeviceDesc.DispName		= "Realtek RTL8723AS Wireless LAN 802.11n SDIO Network Adapter"



;*******************************************************************************
; RTL8723bs Device description
;*******************************************************************************
RTL8723bs.DeviceDesc 				= "Realtek RTL8723BS Wireless LAN 802.11n SDIO Network Adapter"
RTL8723bs.DeviceDesc.DispName		= "Realtek RTL8723BS Wireless LAN 802.11n SDIO Network Adapter"

;*******************************************************************************
; RTL8814as Device description
;*******************************************************************************
RTL8814as.DeviceDesc 				= "Realtek RTL8814AS Wireless LAN 802.11ac SDIO Network Adapter"
RTL8814as.DeviceDesc.DispName		= "Realtek RTL8814AS Wireless LAN 802.11ac SDIO Network Adapter"

;*******************************************************************************
; RTL8188ES Device description
;*******************************************************************************
RTL8188es.DeviceDesc 				= "Realtek RTL8189ES Wireless LAN 802.11n SDIO Network Adapter"
RTL8188es.DeviceDesc.DispName		= "Realtek RTL8189ES Wireless LAN 802.11n SDIO Network Adapter"
;*******************************************************************************
; RTL8821as Device description
;*******************************************************************************
RTL8821as.DeviceDesc 			= "Realtek RTL8821AS Wireless LAN 802.11ac SDIO Network Adapter"
RTL8821as.DeviceDesc.DispName		= "Realtek RTL8821AS Wireless LAN 802.11ac SDIO Network Adapter"
;*******************************************************************************
; RTL8192E Device description
;*******************************************************************************
RTL8192es.DeviceDesc 				= "Realtek RTL8192ES Wireless LAN 802.11n SDIO Network Adapter"
RTL8192es.DeviceDesc.DispName		= "Realtek RTL8192ES Wireless LAN 802.11n SDIO Network Adapter"

;*******************************************************************************
; RTL8703bs Device description
;*******************************************************************************
RTL8703bs.DeviceDesc 				= "Realtek RTL8703BS Wireless LAN 802.11n SDIO Network Adapter"
RTL8703bs.DeviceDesc.DispName		= "Realtek RTL8703BS Wireless LAN 802.11n SDIO Network Adapter"

;*******************************************************************************
; RTL8188Fs Device description
;*******************************************************************************
RTL8188fs.DeviceDesc 				= "Realtek RTL8189FTV Wireless LAN 802.11n SDIO Network Adapter"
RTL8188fs.DeviceDesc.DispName		= "Realtek RTL8189FTV Wireless LAN 802.11n SDIO Network Adapter"
;*******************************************************************************
; RTL8822bs Device description
;*******************************************************************************
RTL8822bs.DeviceDesc 			= "Realtek RTL8822BS Wireless LAN 802.11ac SDIO Network Adapter"
RTL8822bs.DeviceDesc.DispName		= "Realtek RTL8822BS Wireless LAN 802.11ac SDIO Network Adapter"

;*******************************************************************************
; RTL8821cs Device description
;*******************************************************************************
RTL8821cs.DeviceDesc 			= "Realtek RTL8821CS Wireless LAN 802.11ac SDIO Network Adapter"
RTL8821cs.DeviceDesc.DispName		= "Realtek RTL8821CS Wireless LAN 802.11ac SDIO Network Adapter"


;*******************************************************************************
; RTL8723ds Device description
;*******************************************************************************
RTL8723ds.DeviceDesc 				= "Realtek RTL8723DS Wireless LAN 802.11n SDIO Network Adapter"
RTL8723ds.DeviceDesc.DispName		= "Realtek RTL8723DS Wireless LAN 802.11n SDIO Network Adapter"
